COSHH ASSESSMENT

NCS/FM/070 Issue005/Jul09

Ref: COSHH 08

 Assessed by: Matt Traynor Position: Managing Director

Date: January 2022

Reviewed by: Matt Traynor

Position: Managing Director

Date: January 2022

Issue: 008/January 22

Trade name / Supplier: Telephone number:

Contact:

Toxic Corrosive

Product type:

Handling of Cement

Irritant

Highly

Flammable

Chemicals and appearances:

Odorless fine white to grey powder

Harmful

Oxidising

|  |  |
| --- | --- |
| Risk associated with use: | Cement dust acts as a skin and respiratory irritant. Dust and wet cement act as a serious irritant |
|  |  |
| Personal Protection: | Dust proof goggles should be worn, whenever there is a risk of wet mix entering the eyes. Protective clothing should be worn, including waterproof gloves, trousers and appropriate footwear |
|  |  |
| Storage:Store in dry conditi | ons, preferably above ground on pallets protected by shrink wrapping - this will prevent moisture ingress and prolong shelf life |
|  |  |
| Disposal: | Dispose of empty bags or material at an authorised disposal site |
|  |  |
| Fire: | Not flammable |

Appointment Effect First Aid

Dermatitis, irritation, redness, pain

Skin

Wash well with plenty of soap and water for at least 15 minutes

Remove contaminated clothing. Seek medical advice. Wash clothing before re-use

Irritation, stinging Flush eyes with copious quantity of water.

Eyes

If irritation persists, seek medical advice

Inhalation Irritation to nose and throat. Move to fresh air and rest. If symptoms persist seek medical advice

Nausea, Do not Induce vomiting. Wash out mouth with water. Seek medical advice if deemed necessary

Swallowing

